{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Objekt"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":37,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Objekt","index":0,"n_rows":76,"n_cols":24,"rows_kept":76,"cut":false,"hidden":false,"merged":[[12,12,12,13],[24,12,24,13],[30,12,30,13]]}
["Objektdaten:",null,"EFH in",null,null,"__________________"]
[]
["Regenwasser"]
[]
["Regenwasseranfall",null,"Faktor",null,"GG","1. UG","EG","1. OG","2. OG","3. OG","4. OG",null,"Total\nm2",null,"r =","Total","l/s"]
["Hartbelag",null,1,null,null,null,null,62.3,89.3,null,null,null,{"$f":"SUM(E6:L6)","v":151.6},null,0.03,{"$f":"O6*C6*M6","v":4.548},"l/s"]
["begrünt",null,0.3,null,null,null,null,null,null,null,null,null,{"$f":"SUM(E7:L7)","v":0},null,0.03,{"$f":"O7*C7*M7","v":0},"l/s"]
["Garagerampe",null,1,null,null,null,null,null,null,null,null,null,{"$f":"SUM(E8:L8)","v":0},null,0.03,{"$f":"O8*C8*M8","v":0},"l/s"]
[]
["Total Volumenstrom",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(M6:M8)","v":151.6},"m2",null,{"$f":"SUM(P6:P8)","v":4.548},"l/s"]
[]
[]
["Regenwassernutzung","WAR\n(LU)",null,null,"GG","1. UG","EG","1. OG","2. OG","3. OG","4. OG",null,"Apparate",null,"Total\nWAR"]
["Gartenventil (WAR)",5,null,null,null,1,1,null,null,null,null,null,{"$f":"SUM(E14:L14)","v":2},null,{"$f":"IF(M14=0,\"\",B14*M14)","v":10},null,null,null,{"$f":"IF(O14=\"\",0,O14/$M14)","v":5}]
["WC (WAR)",1,null,null,null,null,null,1,null,null,null,null,1,null,{"$f":"IF(M15=0,\"\",B15*M15)","v":1},null,null,null,{"$f":"IF(O15=\"\",0,O15/$M15)","v":1}]
["Urinoir (WAR)",3,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"IF(M16=0,\"\",B16*M16)","v":""},null,null,null,{"$f":"IF(O16=\"\",0,O16/$M16)","v":0},null,null,"Diagramm 1"]
["Waschmaschine (WAR)",2,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"IF(M17=0,\"\",B17*M17)","v":""},null,null,null,{"$f":"IF(O17=\"\",0,O17/$M17)","v":0},null,null,"LU","KW","WW"]
[]
["Total",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(M14:M17)","v":3},"Stk.",{"$f":"SUM(O14:O17)","v":11},"BW",null,null,{"$f":"MAX(S14:S17)","v":5},null,null,3,{"$f":"0.459*POWER(O19/10,0.353)","v":0.47470554356672129}]
["Total Volumenstrom (gemäss Gleichzeitigkeitsdiagramm W3d, S.17, max. 5'000 BW)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($O$61<300,VLOOKUP(S19,V19:W20,2),0.459*POWER($O$61/10,0.353))","v":0.61282871141515627},"l/s",null,null,null,null,null,5,{"$f":"0.598*POWER(O19/10,0.257)","v":0.61282871141515627}]
[]
[]
["Trinkwasser"]
[]
["Apparate","WKN\n(LU)","WAR\n(LU)",null,"GG","1. UG","EG","1. OG","2. OG","3. OG","4. OG",null,"Apparate",null,"Total\nWKN","Total\nWAR"]
["Gartenventil Netzdruck",5,null,null,null,null,1,null,null,null,null,null,{"$f":"SUM(E26:L26)","v":1},null,{"$f":"$B26*M26","v":5},null,null,null,{"$f":"IF(M26=0,0,O26/M26)","v":5}]
["Total",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(M26:M26)","v":1},"Stk.",{"$f":"SUM(O26:O26)","v":5},"BW"]
["Total Volumenstrom (gemäss Gleichzeitigkeitsdiagramm W3d, S.17, max. 5'000 BW)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($O$27<300,0.598*POWER($O$27/10,0.257),0.459*POWER($O$27/10,0.353))","v":0.50042209312466812},"l/s"]
[]
[]
["Apparate","WKR\n(LU)","WWV\n(LU)","WAS\n(DU)","GG","1. UG","EG","1. OG","2. OG","3. OG","4. OG",null,"Apparate",null,"Total\nWKR","Total\nWWV","Total\nWAS"]
["Küche",3,2,0.8,null,null,1,null,null,null,null,null,{"$f":"SUM(E32:L32)","v":1},null,{"$f":"IF(M32=0,\"\",B32*M32)","v":3},{"$f":"IF(M32=0,\"\",C32*M32)","v":2},{"$f":"IF(M32=0,\"\",D32*M32)","v":0.8},null,{"$f":"IF(O32=\"\",0,O32/$M32)","v":3},{"$f":"IF(P32=\"\",0,P32/$M32)","v":2}]
[]
["WC",1,null,2.5,null,null,null,null,null,null,null,null,{"$f":"SUM(E34:L34)","v":0},null,{"$f":"IF(M34=0,\"\",B34*M34)","v":""},null,{"$f":"IF(M34=0,\"\",D34*M34)","v":""},null,{"$f":"IF(O34=\"\",0,O34/$M34)","v":0},0]
["Waschtisch",1,1,0.5,null,null,null,null,null,null,null,null,{"$f":"SUM(E35:L35)","v":0},null,"",{"$f":"IF(M35=0,\"\",C35*M35)","v":""},"",null,0,0]
[]
["Badewanne",3,3,0.8,null,null,1,null,null,null,null,null,{"$f":"SUM(E37:L37)","v":1},null,3,3,0.8,null,3,3]
["WC",1,null,2.5,null,null,1,null,null,null,null,null,{"$f":"SUM(E38:L38)","v":1},null,1,null,2.5,null,1,0]
["Waschtisch",1,1,0.5,null,null,1,null,null,null,null,null,{"$f":"SUM(E39:L39)","v":1},null,1,1,0.5,null,1,1]
[]
["Duschenwanne",2,2,0.6,null,null,null,1,null,null,null,null,1,null,2,2,0.6,null,2,2]
["WC",1,null,2.5,null,null,null,1,null,null,null,null,{"$f":"SUM(E42:L42)","v":1},null,1,null,2.5,null,1,0]
["Waschtisch",1,1,0.5,null,null,null,1,null,null,null,null,{"$f":"SUM(E43:L43)","v":1},null,1,1,0.5,null,1,1]
[]
["Waschtrog",2,2,0.8,null,1,null,null,null,null,null,null,1,null,2,2,0.8,null,2,2]
["Waschmaschine",2,null,0.8,null,1,null,null,null,null,null,null,1,null,2,null,0.8,null,2,0]
[]
["Gartenhahn Terrasse",2,null,null,null,null,null,null,null,null,null,null,0,null,"",null,"",null,0,0]
[]
["Ausgussbecken",2,2,0.8,null,null,null,null,null,null,null,null,{"$f":"SUM(E50:L50)","v":0},null,{"$f":"IF(M50=0,\"\",B50*M50)","v":""},{"$f":"IF(M50=0,\"\",C50*M50)","v":""},{"$f":"IF(M50=0,\"\",D50*M50)","v":""},null,0,0]
["Urinal wasserlos",null,null,0.8,null,null,null,null,null,null,null,null,0,null,"",null,"",null,0,0]
["Urinal",3,null,0.8,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0]
["Bidet",1,1,0.5,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0]
[]
["Secomat",null,null,0.1,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0]
["BA 56",null,null,1,null,null,null,null,null,null,null,null,{"$f":"SUM(E56:L56)","v":0},null,"","","",null,0,0]
["BA 70",null,null,1.5,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0]
["BA 110",null,null,2.5,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0,null,"Diagramm 1"]
["___",null,null,null,null,null,null,null,null,null,null,null,0,null,"","","",null,0,0,null,"LU","KW","WW"]
[]
["Total",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(M37:M59)","v":8},"Stk.",{"$f":"SUM(O32:O59)","v":16},{"$f":"SUM(P32:P59)","v":11},"LU",null,{"$f":"MAX(S32:S59)","v":3},{"$f":"MAX(T32:T59)","v":3},null,3,{"$f":"0.459*POWER(O61/10,0.353)","v":0.54183498056792667},{"$f":"0.459*POWER(P61/10,0.353)","v":0.47470554356672129}]
["Total Volumenstrom (gemäss Gleichzeitigkeitsdiagramm W3d, S.17, max. 5'000 BW)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($O$61<300,VLOOKUP(S61,V61:X62,2),0.459*POWER($O$61/10,0.353))","v":0.54183498056792667},{"$f":"IF($P$61<300,VLOOKUP(T61,V61:X62,3),0.459*POWER($P$61/10,0.353))","v":0.47470554356672129},"l/s",null,null,null,null,5,{"$f":"0.598*POWER(O61/10,0.257)","v":0.67477660913482029},{"$f":"0.598*POWER(P61/10,0.257)","v":0.61282871141515627}]
[]
[]
[]
["Total",null,null,null,null,null,null,null,null,null,null,null,{"$f":"M61+M27","v":9},"Stk.",{"$f":"O27+O61+P61+O19","v":43},"LU",null,null,{"$f":"MAX(S26:S59)","v":5},null,null,3,{"$f":"0.459*POWER(O66/10,0.353)","v":0.76811642220642806}]
["Total Volumenstrom (gemäss Gleichzeitigkeitsdiagramm W3d, S.17, max. 5'000 BW)",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($O$66<300,VLOOKUP(S66,V66:X67,2),0.459*POWER($O$66/10,0.353))","v":0.86996659536944754},"l/s",null,null,null,null,null,5,{"$f":"0.598*POWER(O66/10,0.257)","v":0.86996659536944754}]
[]
[]
["Schmutzabwasser (WAS)"]
[]
[]
["Total Volumenstrom (gemäss 0.5 * WURZEL(DU) oder max. Wert)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(Q32:Q59)","v":9.8000000000000007},"DU",null,{"$f":"IF(M73<60,0.5*SQRT(60),0.5*SQRT(M73))","v":3.872983346207417},"l/s"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(M76=0,\"\",B76*M76)","v":""}]